SECTION 28 23 29

H.265 8 MEGAPIXEL (SUPERIOR HD) TRUE DAY/NIGHT IR RUGGED MULTI-IMAGER IP BULLET CAMERA

1. GENERAL
   1. SECTION INCLUDES
      1. Provide a high definition 8 megapixel (Superior HD) TDN, IR multi-imager rugged outdoor IP bullet camera system with four (4) fixed lenses for video surveillance, including design, supply, installation, and commissioning.
   2. RELATED SECTIONS

NOTE TO SPECIFIER: Include related sections as appropriate if video surveillance system is integrated to other systems.

* + 1. Section 26 05 00: Common Work Results for Electrical, for interface and coordination with building electrical systems and distribution.
    2. Section 28 05 13: Conductors and Cables for Electronic Safety and Security, for cabling between system servers, panels, and remote devices.
    3. Section 28 05 28: Pathways for Electronic Safety and Security, for conduit and raceway requirements.
    4. Section 28 23 00: Video Surveillance Equipment, for interface with, and administration of video recording equipment.
    5. Section 28 23 23: Video Surveillance Systems Infrastructure.
    6. Section 28 23 29: Video Surveillance Remote Devices and Sensors.
  1. REFERENCES
     1. Reference Standards: Provide systems that meet or exceed the requirements of the following publications and organizations as applicable to the work of this Section.
        1. Canadian ICES-003.
        2. Canadian Standards Association (CSA).
        3. Conformity for Europe (CE).
        4. Electronic Industry Association (EIA).
        5. Federal Communications Commission (FCC).
        6. Institute of Electronic and Electrical Engineers (IEEE).
        7. Joint Photographic Experts Group (JPEG).
        8. National Television Systems Committee (NTSC).
        9. Phase Alternating Line (PAL).
        10. Underwriters Laboratories Inc. (UL).
        11. IP Code (Ingress Protection Rating) per IEC 60529.
  2. SYSTEM DESCRIPTION
     1. The 8 megapixel (Superior HD) TDN IR rugged outdoor multi-imager IP bullet camera, HMBL8GR1, shall provide:
        1. Superior Image Quality
           1. Superior HD 8 megapixel (4096 × 1800) resolution, 1–25 fps image with four (4) 1/2.8" 2 megapixel progressive scan CMOS sensors.
           2. Digital WDR, ensuring glare-free images.
           3. True day/night functionality providing vivid color images by day and clear black-and-white images at night with ICR.
           4. Excellent low-light performance with 3D noise reduction, and together with H.265 Profile codec saving storage and bandwidth.
        2. Flexible Surveillance Solution
           1. Four (4) 3.0 mm, M12, fixed lenses.
           2. H.265, H.264 and MJPEG codec with triple stream support.
           3. IR LEDs provide up to 98 ft (30 m) of illumination in dimly lit or nighttime scenes (depending on scene reflectance).
           4. Smart IR technology provides even distribution of IR light.
           5. Waterproof (IP67) and IK10 vandal resistant camera housing.
           6. –40°F to 140°F (–40°C to 60°C) working temperature.
           7. ONVIF™ Profile S, G and Q support.
           8. Security features include individual signed certificates and data encryption.
           9. Cameras can be retrofitted on many existing DVR/NVR installations without requiring additional storage.
        3. Easy to Install and Use
           1. Built-in PoE (Power over Ethernet) eliminates separate power supply and associated wiring; 24 V AC inputs where PoE power is unavailable.
           2. Remote configuration and auto focus through web client or from the NVR.
           3. Included accessories: security screw driver, 4S mount adapter, rubber gasket, and conduit adapter.
        4. Onboard Video Storage
           1. Supports up to 128 GB microSDHC (Class 10) card for local video storage when network is interrupted. Card not included.
  3. SUBMITTALS
     1. General: Submittals shall be made in accordance with the Conditions of the Contract and Submittal Procedure Section.
     2. Manufacturer’s Product Data: Submit manufacturer’s data sheets indicating systems and components proposed for use, including instruction manuals.
     3. Shop Drawings: Submit installation drawings, including connection diagrams for interfacing equipment, list of connected equipment, and locations for major equipment components. Shop drawings shall indicate surrounding construction as provided for the Project.
     4. Project Record Drawings: Indicate location of equipment and wiring on project record drawings. Submit an electronic version of the project record drawings not later than Substantial Completion of the Project.
     5. Operation and Maintenance Data: Submit manufacturer’s operation and maintenance data customized to the system installed. Include operator manuals.
     6. Field Tests: Submit results of field testing of every device, including date, testing personnel, retesting date (if applicable), and confirmation that every device passed field testing.
     7. Maintenance Service Agreement: Submit a sample copy of the manufacturer’s maintenance service agreement, including cost and services for a one year period for Owner’s review. Maintenance shall include, but not be limited to, labor and materials to repair the system, tests and adjustments, and regular inspections.
  4. QUALITY ASSURANCE
     1. Manufacturer: Minimum 10 years experience in manufacturing and maintaining video surveillance systems. Manufacturer shall provide toll-free technical assistance and support available 24/7.
     2. Manufacture Location: Provide equipment assembled in China.
     3. Installer: Minimum 2 years experience installing similar systems and shall be acceptable to the manufacturer of the video surveillance system.
     4. Regulatory Requirements:
        1. Emissions: EN 55032; ANSI C63.4-2014; ICE 003 Rev6; AS/NZ CISPR 32:2013.
        2. Immunity: CE - EN 50130-4.
        3. Safety: North America UL Listed to UL/CSA 60950-1; CE – EN 60950-1.  
            North America UL Listed to UL/CSA 60950-22; CE – EN 60950-22.
     5. Environmental Requirements:
        1. Operating temperatures shall be between –40°F (−40°C) and 140°F (60°C).
        2. Relative Humidity: Less than 95%, non-condensing.
        3. Ingress Protection: IP67.
        4. Vandal Resistance: IK10.
     6. Power Requirements:
        1. Input Voltage: 24 V AC +/-10%, PoE+ IEEE 802.3at.
        2. Power Consumption: PoE+ (802.3at) Class 4, 24 V AC 25 W max (IR LEDs on).
  5. DELIVERY, STORAGE, AND HANDLING
     1. Packing and Shipping: Deliver products in manufacturer’s labeled packages.
     2. Storage and Protection: Store and handle products in accordance with manufacturer’s requirements, in a facility where environmental conditions are within recommended limits.
  6. WARRANTY
     1. Manufacturer’s Guarantee: Five (5) years from the manufacture date code under normal use and service for the video surveillance system.

1. PRODUCTS
   1. MANUFACTURERS
      1. Specified Manufacturer: Honeywell 8 megapixel low light IR rugged multi-imager IP bullet camera, [www.honeywell.com](http://www.honeywellvideo.com)/security.
      2. Accepted Part Numbers:
         1. HMBL8GR1: Network TDN Low Light IR Rugged Multi-Imager Bullet Camera,   
            4 x 1/2.8" CMOS, 8 MP, 4 x 3.0 mm M12 fixed lenses, 8 IR LEDs, PoE+, H.265.
   2. SYSTEM COMPONENTS
      1. 8 megapixel low light, IR rugged outdoor multi-imager IP bullet camera, camera housing, cabling, and a web based GUI that provides complete control of camera settings and live video access.
   3. OPERATIONAL REQUIREMENTS
      1. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall meet or exceed the following camera specifications:
         1. Image Sensor: 4 x 1/2.8" 2 MP Progressive CMOS sensors.
         2. Total Pixels: 4096 × 1800.
         3. Minimum Illumination: 0.008 lux color @ F2.1, 0 lux BW with IR LEDs on @ F2.1.
         4. Wide Dynamic Range: Digital WDR.
         5. IR Distance: Up to 98 ft (30 m), depending on scene reflectance.
         6. Number of IR LEDs: 8.
         7. Backlight Compensation: BLC/HLC/DWDR.
         8. Day/Night: Auto (ICR)/Color/BW.
         9. Gain Control: Auto/Manual.
         10. Noise Reduction: 3DNR.
         11. Privacy Masking: Up to 4 areas.
         12. Electronic Shutter Speed: Auto, Manual, 1/3 to 1/100,000 seconds.
         13. Video Standard: NTSC/PAL.
         14. White Balance: Auto/Natural/Street Lamp/Outdoor/Manual.
         15. Signal-to-Noise Ratio: ≥50 dB.
         16. Audio Stream: Dual stream; Line In/Out.
         17. Audio Compression: G.711a/G.711Mu/AAC/G.726.
         18. Lens: 4 x 3.0 mm, M12, fixed lenses.
         19. Horizontal Angle of View: 180°.
         20. Optimum Installation Distance: > 16.4 ft. (5.0 m), depending on the installation angle and the object size.
         21. Communication: ONVIF Profile S/G/Q support.
      2. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall provide true day/night functionality with an infrared (IR) cut filter for day mode.
      3. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall provide, in high contrast lighting conditions, higher quality images and significantly better dynamic range than conventional IP cameras.
      4. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall provide up to 4 fully configurable privacy zones to mask sensitive areas of a video image.
      5. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall support the ONVIF Profile S/G/Q specification for interoperability between network video products.
      6. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall include, as standard, a web based GUI that provides complete control of the camera settings. The web based GUI shall:
         1. Permit twenty (20) users @ 8 MP resolution at 10 Mbps in simultaneous unicast.
         2. Provide multiple user access levels with password protection.
         3. Offer video access from a web browser. The web browser shall offer live viewing for up to twenty (20) users @ 8 MP resolution at 10 Mbps with full-control of all camera settings available to the administrator.
         4. Be easily discovered through Honeywell IPC Config Tool or other appropriate device search tools.
         5. Be available to record streaming video or snapshot images to a PC hard disk. The administrator must have the ability to turn the recording function on or off through the web based GUI.
         6. Require the following hardware as a minimum for the web browser:
            1. Operating system: Windows 7
            2. Processor: Intel® Pentium® M processor, 2.16 GHz or faster  
                Intel® Core™2 Duo processor, 2.0 GHz or faster
            3. System memory (RAM): 2 GB
            4. Graphics card: AGP graphics card 64 MB RAM, DirectDraw
            5. Network card: 100Base-TX (100 Mbps) or 1000Base-T (1000 Mbps) operation
            6. Web browser: Microsoft Internet Explorer 11.0 or later, Firefox, Chrome
            7. Viewer: ActiveX control plug-in for Internet Explorer
      7. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall support IPv4/v6, HTTP, TCP/IP, DHCP, IGMP, DDNS, RTSP, RTP, RTCP, UDP, FTP, ICMP, SMTP, PPPoE, HTTPS, SSL, UPnP, IEEE 802.1X, IP Filter, Multicast, SNMP v2c/v3, QoS, Bonjour, ONVIF, DNS, and NTP protocols.

NOTE TO SPECIFIER: Some development may be required in specific user cases to support some of these protocols in the field as naturally the protocols will mature over time.

* + 1. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall provide triple H.265, H.264 and/or H.264/MJPEG video streams simultaneously. The streams shall have the following functions:
       1. Main Stream: Support for 8 MP resolution (4096x1800) and lower resolutions at   
          1-25 frames per second: 8M (4096x1800), 3840x1680, 2880x1264 resolutions.
       2. Sub Stream: 1-25/30 fps 1024x452.
       3. Triple Stream: 1-25/30 fps 1920x832, 1280x560.
       4. The 8 MP low light, IR rugged multi-imager IP bullet camera shall transmit additional H.265, H.264 or MJPEG video streams simultaneously with the primary H.265, H.264 or MJPEG stream (up to 3 streams).
       5. The bit rate for the H.265, H.264 and MJPEG streams can be set to constant or variable bit rate. The resolutions and frame rates for all streams are adjustable by the administrator.
       6. The fully featured 8 MP low light, IR rugged multi-imager IP bullet camera shall support three (3) H.264 profiles: High profile, Main profile, and Baseline profile.
    2. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall feature web GUI menus for programming camera parameters. A minimum of the following menus must be available:
       1. Live
       2. Playback
       3. Camera Setup
          1. Properties
          2. Profile Management
       4. Compression Setup
          1. Video
          2. Snapshot
          3. Overlay
          4. ROI
          5. Path
       5. Audio Setup
       6. Network Setup
          1. TCP/IP
          2. Connection
          3. PPPoE
          4. DDNS
          5. IP Filter
          6. SMTP (Email)
          7. UPnP
          8. SNMP
          9. Bonjour
          10. Multicast
          11. 802.1x
          12. QoS
          13. Certificate
       7. Alarm Setup
          1. Alarm
          2. Event
       8. Video Analytics
          1. Video Detection
          2. Face Detection
          3. Audio Detection
       9. Storage Setup
          1. Schedule
          2. Destination
          3. Record Control
       10. System Setup
           1. General
           2. Date&Time
           3. Account
           4. Default
           5. Import/Export
           6. Auto Maintain
           7. Upgrade
       11. Information
           1. Version
           2. Log
           3. Online User
    3. The 8 MP low light, IR rugged multi-imager IP bullet camera system must provide the option of restoring all displays, alarms, camera settings, and diagnostic settings to factory default with a Web GUI command. In addition, the unit shall offer a simple “reboot” with a Web GUI command.
    4. The 8 MP low light, IR rugged multi-imager IP bullet camera system should provide a warning message through relay output/FTP/Email/HTTP, upload an image through FTP/Email or record video to a micro SD card/network recorder upon motion detection. The administrator must have the ability to turn the motion detection function on or off through the web GUI.
    5. The 8 MP low light, IR rugged multi-imager IP bullet camera system should provide a warning message through relay output/FTP/Email, or record video to a micro SD card upon network failure detection, the minimum detecting period is 5 seconds. The administrator must have the ability to adjust the detecting period and turn the network failure detection function on or off through the web GUI.
    6. The 8 MP low light, IR rugged multi-imager IP bullet camera system should provide micro SD card recording for backup when there is an event (Alarm, Motion detection, Network failure detection) or scheduling. The administrator must have the ability to turn the recording function on or off through the web GUI. The micro SD card storage size can be varied from 8 GB to 128 GB. The micro SD card can be inserted, replaced or removed by the installer or the user. The 8 MP low light, IR rugged multi-imager IP bullet camera does not come with a micro SD card installed. It is recommended to use a high quality micro SD card for recording, such as a Class 10 micro SD card.

NOTE TO SPECIFIER: IMPORTANT! Any damaged files on an installed micro SD card incurred by malfunction or error in files saved on the micro SD card, regardless of the cause, are not guaranteed by Honeywell.

* + 1. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall provide Network share recording for backup when there is an event (alarm, motion detection) or scheduling. The administrator must have the ability to turn the recording function on or off through the web GUI.
    2. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall record video with 4 fixed 3.0 mm M12 lenses that will be automatically stitched together by internal software algorithms to record and display a 180° panoramic image.
    3. The 8 MP low light, IR rugged multi-imager IP bullet camera shall include two (2) on-board alarm inputs for normally open or normally closed dry contacts.
    4. The 8 MP low light, IR rugged multi-imager IP bullet camera shall include two (2) on-board alarm output for normally open or normally closed dry contacts. The camera shall have the ability to perform the relay out signal to the alarm equipment.
    5. The 8 MP low light, IR rugged multi-imager IP bullet camera housing shall consist of die cast aluminum with a white powder coat finish (RAL9003).
    6. The 8 MP low light, IR rugged multi-imager IP bullet camera shall be available in indoor/outdoor configurations designed for installation with wall, surface, corner, pole and ceiling mount configurations The 8 MP low light, IR rugged multi-imager IP bullet camera units include IP67 ingress protection and IK10 vandal resistance standards.
    7. The 8 MP low light, IR rugged multi-imager IP bullet camera shall be available in a bullet housing specifically designed for installation in an outdoor environment, with an integral resistive type thermostat-controlled heater and blower to maintain a sufficient operating temperature. The housing shall be IP67 rated.
  1. SERIES INTEGRATIONS
     1. The following accessories are compatible with the 8 MP low light, IR rugged multi-imager IP bullet camera:
        1. HDZPMA – Pole Mount Adapter for Wall Mount
        2. HDZCMA – Corner Mount Adapter for Wall Mount
        3. HDZJB – Junction Box
     2. The following NVRs and Hybrid DVRs are compatible with the 8 MP low light, IR rugged multi-imager IP bullet camera:
        1. MAXPRO® NVR Family – Entry to Enterprise Level Network Video Recorders (version 4.50 or greater)
        2. MAXPRO® VMS Family – Entry to Enterprise Level Network Video VMS (version R450 and greater)
        3. DVM – Digital Video Manager (R600.1 SP1)
        4. HUS (5.1)
        5. ONVIF support for interoperability between Honeywell and other manufacturer’s IP-enabled security devices.

NOTE TO SPECIFIER: Some development may be required in specific user cases to support some of these protocols in the field as they mature over time.

* 1. SYSTEM HARDWARE
     1. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall have the following mechanical specifications:
        1. Unit Dimensions (W × H): 11.7 × 6.7 × 4.7 inches (298.0 × 171.0 × 120.0 mm).
        2. Unit Weight: 6.4 lb (2.9 kg).
        3. Optimum Installation Distance: > 16.4 ft. (5.0 m), depending on the installation angle and the object size.
        4. Construction: Die-cast aluminum housing with powder coat.
     2. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall have the following electrical specifications:
        1. Input Voltage: 24 V AC +/-10%, PoE+ IEEE 802.3at Class 4.
        2. Power Consumption: PoE+ (802.3at) Class 4, 24 V AC 25 W max (IR LEDs on).
     3. The 8 MP low light, IR rugged multi-imager IP bullet camera system shall be designed to meet the following environmental conditions:
        1. Operating temperature: –40°F (−40°C) to 140°F (60°C).
        2. Relative Humidity: Less than 95%, non-condensing.
        3. Ingress Protection: IP67.
        4. Vandal Resistance: IK10.
        5. Emissions: EN 55032; ANSI C63.4-2014; ICE 003 Rev6; AS/NZ CISPR 32:2013.
        6. Immunity: CE - EN 50130-4.
        7. Safety: North America UL Listed to UL/CSA 60950-1; CE – EN 60950-1.  
            North America UL Listed to UL/CSA 60950-22; CE – EN 60950-22.
        8. RoHS: EN 50581.
  2. MANUFACTURER SUPPORT
     1. Manufacturer shall provide customer service, pre-sales applications assistance, after-sales technical assistance, access to online technical support, and online training using Web conferencing.
     2. Manufacturer shall provide 24/7 technical assistance and support by means of a toll-free telephone number at no extra charge.

1. EXECUTION
   1. EXAMINATION
      1. Examine site conditions prior to installation. Notify Architect and Owner in writing if unsuitable conditions are encountered. Do not start installation until site conditions are acceptable.
   2. INSTALLATION
      1. All components of the camera system shall be thoroughly tested before shipping to the project location.
      2. Camera system shall be installed, programmed, and tested in accordance with manufacturer’s instructions and recommendations.
         1. Coordinate interfaces with other products with Owner’s representative where appropriate.
         2. Provide conduit, cable, and wire for complete and reliable installation. Obtain Owner’s approval for exact location of cameras, boxes, conduit, cable, and wiring runs prior to installation.
         3. Install conduit, cable, and wire parallel and square with building lines, including raised floor areas. Do not exceed 40 percent fill in conduits. Gather and tie wires for orderly installation.
         4. Coordinate with other trades to provide proper sequencing of installation.
   3. FIELD COMMISSIONING AND CERTIFICATION
      1. Field Commissioning: Test camera system as recommended by manufacturer, including the following:
         1. Conduct complete inspection and testing of equipment, including verification of operation with connected equipment.
         2. Test devices and demonstrate operational features for Owner’s representative and authorities having jurisdiction, as applicable.
         3. Correct deficiencies until satisfactory results are obtained.
         4. Submit written copies of test results.
   4. TRAINING
      1. Conduct on-site system administrator and security/surveillance operator training in accordance with the manufacturer’s instructions and recommendations. Training shall include, but not be limited to: camera administration, provisioning, configuration, operation, and diagnostics.

END OF SECTION