

Honeywell Performance Series Cameras

A&E Specifications

## GENERAL

### SECTION INCLUDES

Provide a high definition camera system for video surveillance, including design, supply, installation, and commissioning.

### RELATED SECTIONS

NOTE TO SPECIFIER: Include related sections as appropriate if video surveillance system is integrated to other systems.

* Section 26 05 00: Common Work Results for Electrical, for interface and coordination with building electrical systems and distribution.
* Section 28 05 13: Conductors and Cables for Electronic Safety and Security, for cabling between system servers, panels, and remote devices.
* Section 28 05 28: Pathways for Electronic Safety and Security, for conduit and raceway requirements.
* Section 28 23 00: Video Surveillance Equipment, for interface with, and administration of video recording equipment.
* Section 28 23 23: Video Surveillance Systems Infrastructure.
* Section 28 23 29: Video Surveillance Remote Devices and Sensors.

### REFERENCES

Reference Standards: Provide systems that meet or exceed the requirements of the following publications and organizations as applicable to the work of this Section.

* Canadian ICES-003.
* Canadian Standards Association (CSA).
* Conformity for Europe (CE).
* Electronic Industry Association (EIA).
* Federal Communications Commission (FCC).
* Institute of Electronic and Electrical Engineers (IEEE).
* Joint Photographic Experts Group (JPEG).
* National Television Systems Committee (NTSC).
* Phase Alternating Line (PAL).
* Underwriters Laboratories Inc. (UL).
* IP Code (Ingress Protection Rating) per IEC 60529.

### SUBMITTALS

General: Submittals shall be made in accordance with the Conditions of the Contract and Submittal Procedure Section.

Manufacturer’s Product Data: Submit manufacturer’s data sheets indicating systems and components proposed for use, including instruction manuals.

Shop Drawings: Submit installation drawings, including connection diagrams for interfacing equipment, list of connected equipment, and locations for major equipment components. Shop drawings shall indicate surrounding construction as provided for the Project.

Project Record Drawings: Indicate location of equipment and wiring on project record drawings. Submit an electronic version of the project record drawings not later than Substantial Completion of the Project.

Operation and Maintenance Data: Submit manufacturer’s operation and maintenance data customized to the system installed. Include operator manuals.

Field Tests: Submit results of field testing of every device, including date, testing personnel, retesting date (if applicable), and confirmation that every device passed field testing.

Maintenance Service Agreement: Submit a sample copy of the manufacturer’s maintenance service agreement, including cost and services for a one year period for Owner’s review. Maintenance shall include, but not be limited to, labor and materials to repair the system, tests and adjustments, and regular inspections.

### DELIVERY, STORAGE, AND HANDLING

Packing and Shipping: Deliver products in manufacturer’s labeled packages.

Storage and Protection: Store and handle products in accordance with manufacturer’s requirements, in a facility where environmental conditions are within recommended limits.

### WARRANTY

Manufacturer’s Guarantee: Three (3) years from the manufacture date code under normal use and service for the video surveillance system.

### QUALITY ASSURANCE

* Manufacturer: Minimum 10 years experience in manufacturing and maintaining video surveillance systems. Manufacturer shall provide toll-free technical assistance and support available 24/7.
* Installer: Minimum 2 years experience installing similar systems and shall be acceptable to the manufacturer of the video surveillance system.

### MANUFACTURER SUPPORT

* Manufacturer shall provide customer service, pre-sales applications assistance, after-sales technical assistance, access to online technical support, and online training using Web conferencing.
* Manufacturer shall provide 24/7 technical assistance and support by means of a toll-free telephone number at no extra charge.

## EXECUTION

### EXAMINATION

Examine site conditions prior to installation. Notify Architect and Owner in writing if unsuitable conditions are encountered. Do not start installation until site conditions are acceptable.

### INSTALLATION

* All components of the camera system shall be thoroughly tested before shipping to the project location.
* Camera system shall be installed, programmed, and tested in accordance with manufacturer’s instructions and recommendations.
  + Coordinate interfaces with other products with Owner’s representative where appropriate.
  + Provide conduit, cable, and wire for complete and reliable installation. Obtain Owner’s approval for exact location of cameras, boxes, conduit, cable, and wiring runs prior to installation.
  + Install conduit, cable, and wire parallel and square with building lines, including raised floor areas. Do not exceed 40 percent fill in conduits. Gather and tie wires for orderly installation.
  + Coordinate with other trades to provide proper sequencing of installation.

### FIELD COMMISSIONING AND CERTIFICATION

Field Commissioning: Test camera system as recommended by manufacturer, including the following:

* + Conduct complete inspection and testing of equipment, including verification of operation with connected equipment.
  + Test devices and demonstrate operational features for Owner’s representative and authorities having jurisdiction, as applicable.
  + Correct deficiencies until satisfactory results are obtained.
  + Submit written copies of test results.

### TRAINING

Conduct on-site system administrator and security/surveillance operator training in accordance with the manufacturer’s instructions and recommendations. Training shall include, but not be limited to camera administration, provisioning, configuration, operation, and diagnostics.

### SYSTEM DESCRIPTION

The WDR 2MP/4MP IR micro-dome camera, H2W4PER3V shall provide:

1. Superior Image Quality
   1. 4M (2688 × 1520); resolution, 1~25/30fps image with a 1/3” 4Megapixel progressive scan CMOS sensor.
   2. WDR, ensuring glare-free images. WDR range: 120dB
   3. True day/night functionality providing vivid color images by day and clear black-and-white images at night with ICR.
   4. Excellent low-light performance with 3D noise reduction, and together with

H.265 Profile codec saving storage and bandwidth.

1. Flexible Surveillance Solution
   1. 2.8 mm, F1.6 Fixed, Board-in
   2. H.265/H.264H/Smart Codec/MJPEG (Sub Stream).
   3. –40°F to 140°F (–40°C to 60°C) working temperature.
   4. ONVIF™ Profile S/G/Q support.
   5. Security features include individual signed certificates and data encryption.
   6. Cameras can be retrofitted on many existing DVR/NVR installations without requiring additional storage.
2. Easy to Install and Use
   1. Built-in PoE (Power over Ethernet) eliminates separate power supply and associated wiring; 12V DC inputs where PoE power is unavailable.
   2. Remote configuration through web client or from the NVR.
3. Onboard Video Storage

Supports up to 256 GB (Micro SDHC) card for local video storage when network is interrupted.

## PRODUCTS

### MANUFACTURERS

1. Specified Manufacturer: Honeywell WDR 2MP/4MP IR micro-dome camera, [www.honeywellvideo.com.](http://www.honeywellvideo.com/)
2. Accepted Part Numbers:

Network WDR 4MP IR Micro Dome Camera, 1/3” CMOS, 2.8 mm Fixed, 8 IR LEDs, PoE, IP66, H.265 / Smart Codec.

### SYSTEM COMPONENTS

WDR 2MP/4MP IR micro-dome camera, camera housing, cabling, and a web-based GUI that provides complete control of camera settings and live video access.

### OPERATIONAL REQUIREMENTS

1. WDR 2MP/4MP IR micro-dome camera system shall meet or exceed the following camera specifications:
   1. Image Sensor:

1/3” 4 Megapixel progressive scan CMOS

* 1. Total Pixels:

2688 × 1520

* 1. Minimum Illumination:

0.005 Lux / F1.6 (Color, 30IRE), 0 Lux / F2.0 (IR ON)

* 1. WDR, ensuring glare-free images. WDR range: 120 dB with Scene Adaptive Control
  2. Backlight Compensation: BLC/HLC/WDR
  3. Day/Night: Auto (ICR)/Color/BW.
  4. Gain Control: 0-100.
  5. Noise Reduction: 3D DNR.
  6. Privacy Masking: Up to 4 areas.
  7. Electronic Shutter Speed: Auto, Manual, 1/ 3~1/ 100000s.
  8. Video Standard: NTSC/PAL.
  9. White Balance: Auto/Natural/Street Lamp/Outdoor/Manual/Customized Region.
  10. Signal-to-Noise Ratio: More than 50dB.
  11. Lens: 2.8 mm, F1.6 Fixed, Board-in
  12. Angle of View: H:103°, V:55°
  13. Communication: ONVIF Profile S/G/Q support.

1. WDR 2MP/4MP IR micro-dome camera system shall provide true day/night functionality with an infrared (IR) cut filter for day mode.
2. WDR 2MP/4MP IR micro-dome camera system shall provide, in high contrast lighting conditions, higher quality images and significantly better dynamic range.
3. WDR 2MP/4MP IR micro-dome camera system shall provide up to 4 fully configurable privacy zones to mask sensitive areas of a video image.
4. WDR 2MP/4MP IR micro-dome camera system shall support the ONVIF Profile S/G/Q specification for interoperability between network video products.
5. WDR 2MP/4MP IR micro-dome camera system shall include, as standard, a web-based GUI that provides complete control of the camera settings. The web-based GUI shall:
6. Provide multiple user access levels with password protection.
7. Be easily discovered through Honeywell IPC Config Tool or other appropriate device search tools.
8. Be available to record streaming video or snapshot images to a PC hard disk. The administrators have the ability turning the recording function on or off through the web-based GUI.
9. Require the following hardware as a minimum for the web browser:
   1. Operating system: Windows 7, Windows 10
   2. Processor:
      * Intel® Pentium® M processor, 2.16 GHz or faster
      * Intel® Core™2 Duo processor, 2.0 GHz or faster
   3. System memory (RAM): 2 GB
   4. Graphics card: AGP graphics card 64 MB RAM, DirectDraw
   5. Network card: 10Base-T (10 Mbps) or 100Base-TX (100 Mbps) operation
   6. Web browser: Microsoft Internet Explorer 11.0
   7. Viewer: ActiveX control plug-in for Internet Explorer
10. WDR 2MP/4MP IR micro-dome camera system shall support HTTP; HTTPs; TCP; ARP; RTSP; RTP; RTCP; UDP; SMTP; DHCP; DNS; PPPoE; IPv4/v6; QoS; UPnP; NTP; Bonjour; IEEE 802.1x; Multicast; ICMP; IGMP; TLS protocols.

NOTE TO SPECIFIER: Some development may be required in specific user cases to support some of these protocols in the field as naturally the protocols will mature over time.

1. WDR 2MP/4MP IR micro-dome camera system shall provide H.265, H.264 or MJPEG triple video streams simultaneously. The streams shall have the following functions:
2. Main Stream:

Support for 2688 × 1520 / 2304 × 1296 / 1920 × 1080 / 1280 × 960 / 1280 × 720@ (1 ~ 25/30fps)

1. Sub Stream:

Support for 704 × 576 / 640 × 480 / 352 × 288@ (1 ~ 25fps) ;

704 × 480 / 640 × 480 / 352 × 240@ (1 ~ 30fps)

Third Stream:

Support for 1280 × 720 / 704 × 576 / 640 × 480

@ (1 ~ 25fps); 1280 × 720 / 704 × 480 / 640 × 480

@ (1 ~30 fps)

1. WDR 2MP/4MP IR micro-dome camera shall transmit additional H.265, H.264 or MJPEG video streams simultaneously with the primary H.265, H.264 or MJPEG stream (up to triple streams).
2. The bit rate for the H.265, H.264 and MJPEG streams can be set to constant or variable bit rate. The resolutions and frame rates for all streams are adjustable by the administrator.
3. WDR 2MP/4MP IR micro-dome camera system shall feature web GUI menus for programming camera parameters. A minimum of the following menus must be available:
4. Live
5. Playback
6. Camera Setup
   1. Conditions
   2. Profile Management
7. Video
   1. Video
   2. Snapshot
   3. Overlay
   4. ROI
   5. Path
8. Network Setup
   1. TCP/IP
   2. Port
   3. PPPoE
   4. SMTP (Email)
   5. UPnP
   6. SNMP
   7. Bonjour
   8. Multicast
   9. 802.1x
   10. Firewall
   11. QoS
   12. Certificate
9. Video Analytics
   1. Video Detection
   2. Smart Plan
   3. IVS
   4. Face Detection
   5. Abnormality
10. Storage Setup
    1. Schedule
    2. Destination
    3. Record Control
11. System Setup
    1. General
    2. Account
    3. Default
    4. Import/Export
    5. Auto Maintain
    6. Upgrade
12. Information
    1. Version
    2. Log
    3. Online User
13. WDR 2MP/4MP IR micro-dome camera system must provide the option of restoring all displays, alarms, camera settings, and diagnostic settings to factory default with a Web GUI command. In addition, the unit shall offer a simple “reboot” with a Web GUI command.
14. WDR 2MP/4MP IR micro-dome camera system should provide a warning message through relay output/sFTP/Email/HTTP, upload an image through sFTP/Email or record video to a micro SD card/network recorder upon motion detection/audio detection/face detection. The administrators have the ability turning the motion detection/audio detection/face detection function on or off through the web GUI.
15. WDR 2MP/4MP IR micro-dome camera system should provide a warning message through relay output/sFTP/Email, or record video to a micro SD card upon network failure detection. Administrators have ability to adjust the detecting period and turn the network failure detection function on or off through the web GUI.

NOTE TO SPECIFIER: IMPORTANT! Any damaged files on an installed micro SD card incurred by malfunction or error in files saved on the micro SD card, regardless of the cause, are not guaranteed by Honeywell.

1. WDR 2MP/4MP IR micro-dome camera system shall provide Network share recording for backup when there is an event (motion detection, network disconnection…) or scheduling. The administrator must have the ability to turn the recording function on or off through the web GUI.
2. WDR 2MP/4MP IR micro-dome camera system shall provide event analytics capability. It shall detect the event of No SD card, SD card error, SD card capacity warning, network disconnection, IP conflict, illegal access. Once an event is detected, it shall trigger one of following linkages in camera.
3. Snapshot in SD
4. Recording in SD
5. Email
6. Local output
7. WDR 2MP/4MP IR micro-dome camera housing shall consist of die cast aluminum with a white powder coat finish (RAL9003).

### SERIES INTEGRATIONS

1. The following accessories are compatible with WDR 2MP/4MP IR micro-dome camera:
   1. HQA-BB3 Junction Box, 2" dome & IR Ball Perf IP Camera
   2. HQA-WK2 Wall Mount bracket, 2" dome& IR Ball Perf IP Camera
   3. HQA-PK HQA 4K Dome Pendant Mount cap
   4. HQA-PM2 Pole Mount Kit, Perf HQA Cam
   5. HQA-CB Ceiling Mount Bracket
   6. HQA-CBE Ceiling Mount Extend
2. The following NVRs and Hybrid DVRs are compatible with WDR 2MP/4MP IR micro-dome camera:

NVR Performance Series NVR (HEN\*\*\*\*3, HEN\*\*\*\*4)

NOTE TO SPECIFIER: Some development may be required in specific user cases to support some of these protocols in the field as they mature over time.

### SYSTEM HARDWARE

1. WDR 2MP/4MP IR micro-dome camera system shall have the following mechanical specifications:

1. Unit Dimensions: Ø106mm×50.3mm (4.17” × 1.98”)

1. Product Weight: Approx. 0.32kg (0.71lb)
2. Material: Metal.
3. WDR 2MP/4MP IR micro-dome camera system shall have the following electrical specifications:
   1. Input Voltage: 12 V DC +/-10%, PoE IEEE 802.3af Class 0.
   2. Power Consumption: PoE IEEE 802.3af Class0, DC 12V<5.7W.
4. WDR 2MP/4MP IR micro-dome camera system shall be designed to meet the following environmental conditions:
   1. Operating temperature:

–40°F (−40°C) to 140°F (60°C).

* 1. Relative Humidity: Less than 95%, non-condensing.
  2. Emissions: FCC Part 15B, EN55032
  3. Immunity: EN 50130-4

5. Safety: UL 60950-1, EN 62368-1

6. RoHS: EN 50581.

END OF SECTION